**St Gluvias Parish Council - Drainage Action Plan (outstanding issues in red)**

|  |  |  |
| --- | --- | --- |
| **Issue** | **Date identified** | **Action taken** |
| Gully on far side of bridge in Ponsanooth is not blocked but has significant build up to not far below grill | Dec 14 | Resolved. Inspected 13/03/15. Debris in sump is below outfall so is satisfactory. This gully is pumped out every 6 months |
| Gully outside church on main road in Ponsanooth is blocked | Dec 14 | Inspected the wrong gully on 13/03/15, still requires inspection |
| Ineffective soak away outside 29/31 on main road, Ponsanooth | Dec 14 | Inspected 13/03/15. New drain frame cover has been installed. Approximately 12m of pipework is still to be laid, to take collected water into main line, rather than old soakaway. |
| Post office drainage, fear of back up of surface water through existing pipework into front yard of shop | Dec 14 | Site meeting held 13/03/15. Surface water from Post office does enter Highways gully which shouldn’t really happen. If there was back up in the highways system, it wouldn’t be the liability of Cormac and Cornwall Council as private drainage should not be entering into their highways system. A non-return valve was discussed but whilst this would stop water backing up onto the Post office property, it would also stop surface water draining away from the Post office property. To mitigate against any back up from the highways system, the following was identified.   * The Post office is already identified as a flood hot spot and is regularly checked by Cormac when storms/heavy rain are expected. * Cormac will request and let us know if the 3-4 gullies off the main road around the post office could be added to the 6 month gully clearance schedule. * Cormac has supplied a map of the gullies identified from the survey around the shop, with direction of flows. * Michelle will ask SWW if there is a way that her surface water can be redirected into the foul water system   In addition to the above, the parish council are writing to the Environment Agency to question the validity of the river flooding designation given to the shop. Also Michelle actively seeks to keep the nearby grills clear in heavy rain and has ordered some flood gates - these will not arrive until May. |
| Gully on Speech lane just off the main road reported to parish council as ineffective in heavy rain | Dec 14 | Resolved. Inspected 13/03/15. Very little debris or water found, appeared in good working order. Work had been done here 2 weeks ago after a report from the public. |
| Gully opposite old school building in Ponsanooth on main road reported to parish council as blocked | Dec 14 | Inspected 13/03/15. Work had been done here 2 weeks ago after a report from the public (incident 151827753) Full of water yet very little debris. This is due to be jetted WC 16/03/15.  On 20/3/15 it was jetted and a camera sent down.  It seems to tie in with an old culvert.  However when they tried filling it with water it suddenly started coming out of the bank between St Michaels and Frog hill near the school wall.  More of a worry it also came out of the bank on the left of Sally and Martin Beckett’s drive and down towards the garage! The guys doing the work said it was going beyond their remit and they would report the problem. |
| Drainage pipe from Stag Hunt pub discharges onto road | Mar 15 | No action to be taken. Inspected 13/03/15. Private drainage should not be directed into highways drainage system and existing drainage is historic |
| Gully at Town tanna junction reported to parish council as blocked | Mar 15 | Resolved. Site visited 13/03/15 by VB and AH (Cormac) – recent surfacing works undertaken here and all drainage looks to have been emptied/addressed as part of these works – no blockages witnessed. |
| On left turn to Mylor off B3292, 2 gullies are full of mud to the top (near sign for potatoes) | Mar 15 | Resolved. Site visited 13/03/15 by VB and AH (Cormac) – gullies witnessed to be full of mud debris (understand this is an ongoing issue due to mud/run-off from nearby fields clogging the sumps up) – currently due to be routinely emptied on a rural basis (once a year from April 2015).  Gullies were hand emptied the same day and silt dispersed on verge (+5m away from the gullies). |
| Ditch and gully need clearing at Lower Treluswell where it meets the B3292, where plumbers are based and old brewery. Currently large cardboard box behind the grill | Mar 15 | Resolved. Site visited 13/03/15 by VB and AH (Cormac).  Cardboard box and other foam packaging in grill removed whilst on-site.  No other issues witnessed with this system. |
| Discharge channel that passes under wall of house next to Mill Stream Cottages is blocked and unsatisfactory, identified by Cormac | Mar 15 | Inspected 13/03/15. Cormac will speak to owners about directing the discharge into nearby stream on their property |